|  |  |  |  |
| --- | --- | --- | --- |
| Name |       | Company |       |
| Tel Number |       | Email |       |
| Order Number |       | Date |       |

Please return completed forms to Chiltern Invadex (UK) Limited by email to sales@chilterninvadex.co.uk.

Should you require advice or guidance please call our customer services team on 01869 365500 opt 1.

**Cubicle Model**

****

**100 101 120 120Plus**

[ ]  Standard [ ]  Standard [ ]  Standard ­­ [ ]  Standard

[ ]  WC [ ]  WC [ ]  WC [ ]  WC

**Waste Options Door Options**

**![Side Entry door options (3394) [Converted].jpg]()![Side Entry door options (3394) [Converted].jpg]()**

[ ]  Gravity [ ]  Pumped [ ]  Macerator (additional cost) Bi-fold [ ]  [ ]  Pair [ ]

 (Standard)

**Shower Options (additional cost)**

[ ]  None [ ]  Mira Advance [ ]  Mira Excel Mixer

**Basin Options (WC cubicles only)**

[ ]  Standard plastic basin (filled via shower) [ ]  Ceramic basin & lever taps (additional cost)

**Cubicle Layout**

![SLIMLINE SE (143) [Converted].jpg]()

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  Left PanelRightPanel RearPanel |  | **Left Panel** | **Rear Panel** | **Right panel** |
|  | Panel height | [ ]  Full Height | [ ]  Full Height | [ ]  Full Height |
|  | [ ]  Half Height | [ ]  Half Height | [ ]  Half Height |
|  | Shower control position(full height panel only) | [ ]  Front of panel[ ]  Rear of panel | N/A | [ ]  Front of panel[ ]  Rear of panel |
|  | Basin position (as per shower control unless otherwise requested) | [ ]  | [ ]  | [ ]  |
|  | WC is located on the rear panel |

**Light & Fan Options (additional cost)**

[ ]  None [ ]  Roof light [ ]  Combined roof light & extractor fan

**Seat Options (Standard cubicles only, additional cost)**

Maximum seat load 20st (130kg)

|  |  |  |
| --- | --- | --- |
| **Code** | **Description** |  |
| SHSS4 | Fold up PVC seat | [ ]  |
| SHSS4P | Fold up padded seat | [ ]  Flat Padded [ ]  Aperture\* [ ]  Horseshoe\* |
| SHSS5 | Fold up PVC seat with arms & backrest | [ ]  |
| SHSS5P | Fold up padded seat with arms & backrest | [ ]  Flat Padded [ ]  Aperture\* [ ]  Horseshoe\* |
| \*Where aperture or horseshoe is required select size | [ ]  Small [ ]  Medium [ ]  Large |
| Seat will be positioned on the rear panel, please specify seat height mm  |

**Kit Contents**

Standard cubicles are provided with tray, removable ramp, waste, enclosure, doors and 2x horizontal rails

WC cubicles are provided with tray, removable ramp, waste, enclosure, doors, WC pan, high level external cistern, plastic basin,

1 x vertical rail & 1 x horizontal rail

**Additional requirements**